{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[0,0,0,8],[1,0,1,8],[2,0,13,8],[14,0,14,8],[15,3,15,4],[15,5,15,6],[15,7,15,8],[16,3,16,4],[16,5,16,6],[16,7,16,8],[17,3,17,8],[18,3,18,8],[19,3,19,4],[19,5,19,6],[19,7,19,8],[20,3,20,8]],"flags":["formulas_cached_only"]}
["PYF3两位二通电磁阀外形图及参数"]
["外形尺寸图"]
{"$rows_empty":12}
["详细参数"]
["额定电压","Rataed  voltage",null,"DC3.7V",null,"DC6V",null,"DC12V"]
["额定电流","Rataed  current",null,"＜450",null,"＜300",null,"＜230"]
["排气速度","Exhaust Speed",null,"500CC容器压力从300mmHg降至15mmHg所需时间＜5s"]
["气 密 性","Leakage",null,"＜3 mmHg/min from 300mmHg at 100cc tank."]
["直流阻抗","DC Resistance\nDC Resistance",null,"   ±10%Ω",null,"   ±10%Ω",null,"   ±10%Ω"]
["寿命测试","Life       test",null,"﹥30000 Times (10s on,7s off)"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}