{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[0,0,0,8],[1,0,1,8],[2,0,13,8],[14,0,14,8],[15,1,15,2],[15,3,15,4],[15,5,15,6],[15,7,15,8],[16,1,16,2],[16,3,16,4],[16,5,16,6],[16,7,16,8],[17,1,17,2],[17,3,17,8],[18,1,18,2],[18,3,18,8],[19,1,19,2],[19,3,19,4],[19,5,19,6],[19,7,19,8],[20,1,20,2],[20,3,20,8]],"flags":["formulas_cached_only"]}
["PYSF3-12A两位三通电磁水阀外形图及参数"]
["外形尺寸图"]
{"$rows_empty":12}
["详细参数"]
["额定电压","Rataed  voltage",null,"DC6V",null,"DC12V",null,"DC24V"]
["额定电流","Rataed  current",null,"＜420",null,"＜300",null,"＜230"]
["压力范围","OperationalPressure",null,"MAX14.5PSI(100Kpa)"]
["密 封 性","Leakage",null,"30mmHg压力下＜5.0mL/min "]
["直流阻抗","DC Resistance\nDC Resistance",null,"   30±10%Ω",null,"   50±10%Ω",null,"   75±10%Ω"]
["寿命测试","Life       test",null,"﹥10010 Times (150s on,30s off)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}