{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":9,"rows_kept":21,"merged":[[0,0,0,8],[1,0,1,8],[2,0,11,8],[12,0,12,8],[13,1,13,2],[13,4,13,5],[13,6,13,7],[14,1,14,2],[14,4,14,5],[14,6,14,7],[15,1,15,2],[15,3,15,8],[16,1,16,2],[16,3,16,8],[17,1,17,2],[17,3,17,8],[18,1,18,2],[18,3,18,8],[19,1,19,2],[19,3,19,8],[20,1,20,2],[20,3,20,8]],"flags":["formulas_cached_only"]}
["PYSP370B款水泵外形图及参数"]
["外形尺寸图"]
{"$rows_empty":10}
["详细参数"]
["额定电压","Rataed  voltage",null,"DC3.7V","DC6V",null,"DC12V",null,"DC24V"]
["额定电流","Rataed  current",null,"＜550","＜380",null,"＜250",null,"＜250"]
["充气时间","Inflation  time",null,"＜10s(From 0 to 300mmHg in a 100cc tank)"]
["水体流量","Air        flow",null,"﹥1.1-1.3LPM"]
["最大压力","Pressure",null,"﹥3kfg"]
["气 密 性","Leakage",null,"＜3 mmHg/min from 300mmHg at 100cc tank."]
["噪    音","Noise",null,"＜65dB"]
["寿命测试","Life       test",null,"﹥30000 Times (10s on,7s off)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}